## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Single Click Locking

This option locks the X,Y coordinates as soon as the button-down threshold has been exceeded. All subsequent touch coordinates are then reported to the system with this X,Y value when sent as emulated mouse data.

Normal reporting of X,Y coordinates resumes:

After the click-lock time has been exceeded
If the touch coordinate moves outside the click-lock area
If the touch is removed from the screen