## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Protected Mode Exceptions

Interrupt 5 if the bounds test fails, as described above; #GP(0) for an illegal memory operand effective address in the CS, DS, ES, FS, or GS segments; #SS(0) for an illegal address in the SS segment; #PF(fault-code) for a page fault; #AC for unaligned memory reference if the current privilege level is 3.

The second operand must be a memory operand, not a register. If the BOUND instruction is run with a ModR/M byte representing a register as the second operand, #UD occurs.