## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MCI_AUDIO_LOAD

This structure contains fields for the AUDIO_LOAD function.

    typedef struct _load {

      CHAR FAR      *pbBuffer;  /*  Pointer to buffer. */

      ULONG          ulSize;    /*  Size of DSP code (in bytes). */

      ULONG          ulFlags;   /*  Indicates start or end of operation. */

    } MCI_AUDIO_LOAD;

    typedef   MCI _ AUDIO _ LOAD   FAR   * LPMCI _ AUDIO _ LOAD ;