## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Syntax

Processor-Register:
General-Purpose-Register
Segment-Register
Control-Register
Debug-Register
Test-Register
MMX-Register
Floating-Point-Register
General-Purpose-Register:
8-Bit-Register
16-Bit-Register
32-Bit-Register
8-Bit-Register: one of
AL AH BL BH CL CH DL DH
16-Bit-Register: one of
AX BX CX DX DI SI BP SP
32-Bit-Register: one of
EAX EBX ECX EDX EDI ESI EBP ESP
Segment-Register: one of
CS DS ES FS GS SS
Control-Register: one of
CR0 CR2 CR3 CR4
Debug-Register: one of
DR0 DR1 DR2 DR3 DR4 DR5 DR6 DR7
Test-Register: one of
TR3 TR4 TR5 TR6 TR7
MMX-Register: one of
MM0 MM1 MM2 MM3 MM4 MM5 MM6 MM7
Floating-Point-Register:
ST