## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### OS2_PM_DRV_ENABLE: Subfunction 09h - ResetDCState - Parameters

ulSubfunction (ULONG) - input 09h

pParam1 (PULONG) - input A pointer (pInstance) to the DC instance data.

pParam2 (PLONG) - input Reserved.

rc (LONG) - returns Return codes.

The handling routine should return a LONG integer. Valid values are:

0 Successful
-1 Error