## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMConvertID - Calling Parameters

pID (PULONG) - output The integer value of the device ID. The following are possible values:

Bits[15:0] Three character compressed ASCII EISA ID.

Bits[31:16] Manufacturer-specific function number and revision.

String (PSZ) - output This is a pointer to a 9 character-long string array.

Direction (USHORT) - output Can be one of the following values:

RM_CONVERT_TO_TEXT

RM_CONVERT_TO_ID

rc (APIRET) - returns On systems where the Resource Manager driver is not installed, the library interface code will return RMRC_NOT_INSTALLED.

RMRC_INVALID_PARM_VALUE
RMRC_SUCCESS