## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Setup:

    The following routines handle setup for source and destination software
    BitBlt's eddf_MESSSetUpPatDest11.

    FFBLTSET.ASM
            eddf_MESSSetUpSrcDest16
            eddf_MESSSetUpSrcDest81
            eddf_MESSSetUpSrcDest41
            eddf_MESSSetUpSrcDest11

The following routine handles setup for non-wrapping pattern setup (such as text):

            eddf_MESSSetUpPatDest11

    The following routines handle setup for destination-only blts:

            eddf_MESSSetUpDest16
            eddf_MESSSetUpDest81
            eddf_MESSSetUpDest24
            eddf_MESSSetUpDest41
            eddf_MESSSetUpDest11

    The following routine handles common setup for 4-bit-per-pel pattern
    blts:

            eddf_MESSSetUpDestForPat41