## Using Your DDK

[prev][next][parent][TOC]

### Generic PMI Sample

Driver Description:

The Generic PMI Sample provides INT 10 support with BIOS mode tables and hardware information.

Compilers/Assemblers Required:

         IBM C Set ++ V2.01

Build Instructions:

1.Ensure the necessary compilers and assemblers are installed.

2.Run the SETCMPLR.CMD REXX command file located in the DDK\TOOLS directory. This command initializes environment variables to be used during the build.

e.g., SETCMPLR <MSCpath> <VACpath> <CSETpath> <DDKpath>

    Where <MSCpath> represents the Microsoft C 6.0 install directory
           <VACpath> represents the IBM Visual Age C++ install directory
           <CSETpath> represents the IBM C Set ++ install directory
           <DDKpath> represents the DDK install directory

Note: A period (.) may be substituted for a compiler directory that is not used during the build.

3.Change the directory to DDK\VIDEO\SRC\VIDEO\GENPMI.

4.Invoke NMAKE on the resident makefile.

Files Created By Successful Build:

         Directory:  \DDK\VIDEO\REL\OS2C\RETAIL\BASE\OS2\DLL

         o  GENPMI.DLL