snmp.conf(5)

NAME
snmp.conf - snmp configuration file for cups

DESCRIPTION
The snmp.conf file configures how the standard CUPS network backends (http, https, ipp, ipps, lpd, snmp, and socket) access printer information using SNMPv1 and is normally located in the /etc/cups directory. Each line in the file can be a configuration directive, a blank line, or a comment. Comment lines start with the # character.

The Community and DebugLevel directives are used by all backends. The remainder apply only to the SNMP backend - cups-snmp(8).

DIRECTIVES
The following directives are understood by the CUPS network backends:

Address @IF(name)

Address @LOCAL

Address address
    Sends SNMP broadcast queries (for discovery) to the specified address(es). There is no default for the broadcast address.

Community name
    Specifies the community name to use. Only a single community name may be specified. The default community name is "public".

DebugLevel number
    Specifies the logging level from 0 (none) to 3 (everything). Typically only used for debugging (thus the name). The default debug level is 0.

DeviceURI "regular expression" device-uri [... device-uri]
    Specifies one or more device URIs that should be used for a given make and model string. The regular expression is used to match the detected make and model, and the device URI strings must be of the form "scheme://%s[:port]/[path]", where "%s" represents the detected address or hostname. There are no default device URI matching rules.

HostNameLookups on

HostNameLookups off
    Specifies whether the addresses of printers should be converted to hostnames or left as numeric IP addresses. The default is "off".

MaxRunTime seconds
    Specifies the maximum number of seconds that the SNMP backend will scan the network for printers. The default is 120 seconds (2 minutes).

SEE ALSO
cups-snmp(8), CUPS Online Help (http://localhost:631/help)

COPYRIGHT
Copyright © 2007-2015 by Apple Inc.