Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@GetCur

Version

IBM 5150 and higher

Brief

Get Current Cursor Position and Size

BIOS Interrupt

INT10H: 03H

Family API

VioGetCurPos VioGetCurType

Syntax

@GetCur page

Parameters

page (BYTE) - optional video page number

Return

CH = start scan line
CL = end scan line
DH = row (00h is top)
DL = column (00h is left)