KbdXlate

Bindings:

C:

typedef struct _KBDTRANS { /* kbxl */ UCHAR chChar; /* ASCII character code */ UCHAR chScan; /* Scan code */ UCHAR fbStatus; /* State of the character */ UCHAR bNlsShift; /* Shift status (reserved set to zero) */ USHORT fsState; /* Shift state */ ULONG time; USHORT fsDD; USHORT fsXlate; USHORT fsShift; USHORT sZero; } KBDTRANS; #define INCL_KBD USHORT rc = KbdXlate(XlateRecord, KbdHandle); PKBDTRANS XlateRecord; /* Translation Record */ HKBD KbdHandle; /* Keyboard handle */ USHORT rc; /* return code

MASM:

KBDTRANS struc kbxl_chChar db ? ;ASCII character code kbxl_chScan db ? ;scan code kbxl_fbStatus db ? ;State of the character kbxl_bNlsShift db ? ;shift status (reserved set to zero) kbxl_fsState dw ? ;shift state kbxl_time dd ? kbxl_fsDD dw ? kbxl_fsXlate dw ? kbxl_fsShift dw ? kbxl_sZero dw ? KBDTRANS ends EXTRN KbdXlate:FAR INCL_KBD EQU 1 PUSH@ OTHER XlateRecord ;Translation Record PUSH WORD KbdHandle ;Keyboard handle CALL KbdXlate Returns WORD

This call translates scan codes with shift states into ASCII codes.

KbdXlate (XlateRecord, KbdHandle)

XlateRecord (PKBDTRANS) - input Address of the translation record structure:

chardata (KBDKEYINFO) Character data information structure as defined in KbdCharIn call.

kbdflag (USHORT) See the KbdDDFlagWord call in the “Keyboard Device Driver” section of IBM Operating System/2 Version 1.2 I/O Subsystems And Device Support Volume 1.

xlate (USHORT) Translation flag:

Value	Definition
0	Translation incomplete.
1	Translation complete.

xlatestate1 (USHORT) Identifies the state of translation across successive calls; initially the value should be zero. It may take several calls to this function to complete a character. The value should not be changed unless a new translation is required, that is, reset value to zero.

xlatestate2 (USHORT) See description for xlatestate1.

KbdHandle (HKBD) - input Default keyboard or the logical keyboard.

rc (USHORT) - return Return code descriptions are:

0	NO_ERROR
439	ERROR_KBD_INVALID_HANDLE
445	ERROR_KBD_FOCUS_REQUIRED
447	ERROR_KBD_KEYBOARD_BUSY
464	ERROR_KBD_DETACHED
504	ERROR_KBD_EXTENDED_SG

Remarks

It may take several calls to complete a translation because of accent key combinations, or other complex operations.

The Xlatestate1 and Xlatestate2 are for use by the keyboard translation routines. These fields are reserved and must only be accessed by the caller prior to starting a translation sequence and then they must be set to zero. The KbdXlate function is intended to be used for translating a particular scan code for a given shift state. The KbdXlate function is not intended to be a replacement for the OS/2 system keystroke translation function.