## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 104h - Remarks

The Environment Buffer is not used by this function. The Environment Buffer address is passed as a DWORD of zero. If the Length specified in the Config Data is larger than the maximum possible length, or if the Length is specified as 2 (the length of Length field itself), it is replaced by the largest valid length.