## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Notes

This instruction can be used with a LOCK prefix. The Intel386 DX microprocessor does not implement this instruction. If this instruction is used, you should provide an equivalent code sequence that runs on an Intel386 DX processor as well. See the Intel documentation for details on how to detect a particular processor at runtime.