## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRJINFO2 Field - fsStatus

fsStatus (USHORT) Job status.

To find the job status, use the PRJ_QSTATUS mask:

PRJ_QS_QUEUED Queued
PRJ_QS_PAUSED Paused by a SplHoldJob function
PRJ_QS_SPOOLING Job being created
PRJ_QS_PRINTING Printing (bits 2 through 11 are valid).

For further information, use the PRJ_DEVSTATUS mask:

PRJ_COMPLETE Job complete
PRJ_INTERV Intervention required
PRJ_ERROR Error occurred.
PRJ_DESTOFFLINE Print destination offline
PRJ_DESTPAUSED Print destination paused
PRJ_NOTIFY Alert should be raised
PRJ_DESTNOPAPER Print destination out of paper
PRJ_DESTFORMCHG Printer waiting for form change
PRJ_DESTCRTCHG Printer waiting for cartridge change
PRJ_DESTPENCHG Printer waiting for pen change.

This bit indicates that the job is deleted:

PRJ_DELETED Job deleted.