## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMGetDriverName - Calling Parameters

pRP (PRPINITIN) Pointer to init request packet.

pBuf (PSZ) Pointer to character buffer for device driver name.

size (USHORT) Buffer size.

rc (APIRET) - returns Contents of pBuf will be a null-terminated device driver name. If unable to determine the device driver name, the contents of pBuf will be a zero-length null-terminated string.