## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### VDHGetVPMExcept

Select an item:

    Format
    Parameters
    Return Codes
    Purpose
    Glossary

This function gets the current value from the protected-mode exception table.

    #include mvdm.h

    ULONG    Vector;                  /*  Exception vector number */

    PFPFN    pHandlerAddressPointer;  /*  Pointer to put handler address */

    PBYTE    pFlag;                   /*  Pointer to a flag variable */

    BOOL     rc;

    rc = VDHGetVPMExcept(Vector, pHandlerAddressPointer,

           pFlag);