## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### ACQUIREFB

Structure describing action to take when acquiring the frame buffer.

    typedef struct _ACQUIREFB {

      ULONG     fAFBFlags;     /*  Flag indicating whether bank switching is required. */

      ULONG     ulBankNumber;  /*  Bank number to switch to. */

      RECTL     rctlXRegion;   /*  Rectangle of cursor exclude region. */

    } ACQUIREFB;

    typedef   ACQUIREFB   * PACQUIREFB ;