## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRTINPUTS Field - curCrossFormSize

curCrossFormSize (USHORT) Current size of the form across feed direction.

This value specifies the current size of the media, in the direction of ninety degrees to the feed or motion direction, that can be input from a particular input feature. The units for this measurement are defined by the lengthUnits parameter in the PRTDEVCHAR data structure. If the size is unknown, the printer returns a value of hex 'FFFF.'