## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 102h - Flags

Flags

Defined as follows:

    Bit 0 is reserved and must be Off.

    Bit 1 indicates whether hardware state (mode,

          CLUT, everything except the buffer) is saved.

          OFF = The hardware state is not saved.

          ON  = The hardware state is saved.

    Bit 2 indicates whether the physical display

          is fully saved for session switching.

          OFF = The physical display is not fully saved.

          ON  = The physical display is fully saved.

    Bit 3 indicates whether the physical display

          is partially saved for pop-ups.

          OFF = The physical display is not partially saved.

          ON  = The physical display is partially saved.

    Bits 4 thru 15 are reserved and must be OFF.