## Printer Device Driver

[prev][next][parent][TOC]

### GplDitherRGBtoRGB

Description

This function is a shell for GplDitherRGBtoCMYK. It simply inverts the CMY pDest buffer to RGB for a printer that requires RGB.

Format

    APIRET APIENTRY GplDitherRGBtoRGB( PHDITHER       pdh,

                                       PDITHEREQUEST  pReq

                                       PDITHERESULT   pReply );

Parameters

pdh (PHDITHER) Pointer to the dither handler that was created by GplDitherCreateInstance.

pReq (PDITHEREQUEST) Address of the API's pre-filled request structure.

pReply (PDITHERESULT) Address of the reply structure.

Returns

Success NO_ERROR