## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### SHD_REPORT_INT Return Value - rc

rc (ULONG) Return codes indicating success or type of failure:

NO_ERROR Success.

ERROR_INVALID_FUNCTION Illegal function requested.

ERROR_INVALID_STREAM Invalid stream handle.

ERROR_DEVICE_UNDERRUN There was a device data underrun.

ERROR_DEVICE_OVERRUN There was a device data overrun.

FAILURE Stream-handler-specific error return code.