## Physical Device Driver Reference

[prev][next][parent][TOC]

### PRT_ACTIVATEFONT (48h) - Returns

The error return codes for this function are as follows:

00H Completed successfully
0AH Write fault, if monitor registered and the DevHlp_MonWrite fails
02H Code page is not available
03H No code page function because spooler not started
04H Font ID is not available (verify)
09H Error caused by switcher error, not by input parameters
0AH Error caused by invalid printer name as input
0DH Received code page request when code page switcher not initialized
0FH SFN table full: cannot activate another entry
13H DASD error reading font file
15H DASD error reading font file definition block
17H DASD error while writing to temporary spool file
18H Disk full error while writing to temporary spool file
19H Spool file handle was bad