## Physical Device Driver Reference

[prev][next][parent][TOC]

### Status - TOUCH_DEVDEP_READDATA (53h)

Status Has the following bit-level definitions for RAW mode:

Bit Description

1 Reserved=0

2 Reserved=0

3 Reserved=0

4 Reserved=0

5 Reserved=0

6 1=Channel pegged

7 Reserved=0

8 Reserved=0

9 Reserved=0

A 1=Adjust just occurred

B Reserved=0

C Reserved=0

D Reserved=0

E 1=Offset error

F 1=RAW data