## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRTALERT

Information returned by the BIDI_WAIT_ALERT command.

    typedef struct _PRTALERT {

      ULONG      ulpszPortName;   /*  Name of the port generating the alert. */

      ULONG      ulCategory;      /*  Category of alert being returned. */

      ULONG      ulType;          /*  Type of alert in a given category. */

      BYTE       interpreterID;   /*  Interpreter identifier that returns this alert. */

      BYTE       bReserved;       /*  Reserved; must be 0 (zero). */

      USHORT     usSeverity;      /*  Severity of problem. */

      ULONG      ulValue;         /*  Value associated with the alert. */

      ULONG      ulPrinterJobID;  /*  Printer job identifier if this is a print job core alert. */

      ULONG      ulpszAlertMsg;   /*  Optional alert text. */

    } PRTALERT;

    typedef   PRTALERT   * PPRTALERT ;