## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreOutlinePath Parameter - flOptions

flOptions (ULONG) - input Outline path flags.

Possible values are:

OPTH_NO_CLIPPING_REQD The graphics engine will outline the path without clipping and line attributes set. This value can be used for devices that have hardware support for area fills with at least simple clipping. This output will be sent to the presentation driver via GreDrawLinesInPath for each subpath. This flag should only be used with the graphics engine version number 0x202 or later (see GreQueryEngineVersion).

OPTH_QRY_PATH_POINTS Returns the number of points in a path. The path is not deleted. This flag should only be used with the graphics engine version number 0x202 or later (see GreQueryEngineVersion).