## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### I/O Port Support

The virtual keyboard device driver is responsible for supporting programs that access the keyboard ports directly. These ports provide access to data ports on the hardware that controls I/O to the keyboard. This support is provided primarily for applications that simply read the scan code directly from the port. However, other functions are possible, such as setting the key repeat rate. Repeat rates affect the entire system; per-DOS session repeat rates are not supported. Extended scanner functions, such as providing keyboard pre-controller translation, are not supported; such commands are ignored.