## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### 32-Bit Super VGA Display Driver

The 32-bit Super VGA display driver, like all display drivers, provides hardware- independence for OS/2 application programs needing to perform I/O to a display device. While the general architecture and functionality of the Super VGA driver are the same as the 32-bit VGA driver, there are differences between the two. This chapter concentrates on those differences . See 32-Bit VGA Display Driver for detailed information about 32-bit VGA display drivers.