## Physical Device Driver Reference

[prev][next][parent][TOC]

### TOUCH_DEVDEP_GETDATAREPORTRATE (65h) - Report rate

Report rate Is the maximum rate at which data packets will be returned by the Touch display while the touch contact force exceeds the On-Screen threshold (see TOUCH_DEVDEP_SETTOUCHTHRESHOLD.) The values are:

0 10 reports per second

1 20 reports per second

2 30 reports per second

3 40 reports per second

4 60 reports per second

-1 Driver default value

All other values are reserved.