## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### SrcEXT

This variable contains the default source file name extension that is conditionally appended to the concatenated values of SrcDIR and SrcNAME; the assembler treats the resulting string as the fully qualified input file name. The default value for SrcEXT is ".asm" unless altered by use of the Fes parameterized command line option.

Related Information:

Options
File Names
Fes - Control Source File Extension (SrcEXT)