## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplEnumQueue Return Value - rc

rc (SPLERR) - returns Return code.

NO_ERROR (0) No errors occurred.
ERROR_ACCESS_DENIED (5) Access is denied.
ERROR_NOT_SUPPORTED (50) This request is not supported by the network.
ERROR_BAD_NETPATH (53) The network path cannot be located.
ERROR_INVALID_PARAMETER (87) An invalid parameter is specified.
ERROR_INVALID_LEVEL (124) The level parameter is invalid.
ERROR_MORE_DATA (234) Additional data is available.
NERR_NetNotStarted (2102) The network program is not started.
NERR_BufTooSmall (2123) The API return buffer is too small.
NERR_InvalidComputer (2351) The computer name is invalid.