## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRTOUTPUTS

Information about the installed printr output bins, returned by the BIDI_Q_ OUTPUTBINS command.

    typedef struct _PRTOUTPUTS {

      BYTE       logicalUnit;  /*  Logical unit number for this interpreter. */

      BYTE       bReserved;    /*  Reserved; must be 0 (zero). */

      USHORT     usReserved;   /*  Reserved; must be 0 (zero). */

      BYTE       outputID;     /*  Output identifier. */

      BYTE       positions;    /*  Number of output positions for this output device. */

      BYTE       features1;    /*  Output features support byte 1. */

      BYTE       features2;    /*  Output features support byte 2. */

      ULONG      maxCapacity;  /*  Maximum capacity per output position. */

      ULONG      ulpszOutput;  /*  Output description string. */

    } PRTOUTPUTS;

    typedef   PRTOUTPUTS   * PPRTOUTPUTS ;