## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VCAI_PLAY (67h) - Restore/Play Image to the Screen

Category:
VIDEO_IOCTL_CAT (140)
Function:
VCAI_PLAY (67h)
Description:
Restore/Play Image to the Screen

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format

This IOCtl is used to play back and restore images to a device. The format of the image data pointed to by pImageData is determined by the VCAI_ RESTORE_FORMAT IOCtl and the source and destination image size is determined by the VCAI_SETCAPTRECT If the device supports this command, the CanRestore flag in the VCADEVINFO structure should be set to 1.