## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### EGA.SYS Device Driver

EGA.SYS is a physical device driver that provides support for the EGA register interface in a DOS session. To support advanced graphics modes D, E, F, and 10 in a DOS session, the Mouse Pointer Draw device driver must save or restore the EGA registers. Because the EGA registers are not readable, this can be done only if the application assists in setting the registers initially. Rather than performing I/O directly to the registers on the adapter, the application sets the registers through the EGA register interface.