## Graphics Adapter Device Driver Reference

[prev][next][parent][TOC]

### VRAMALLOCOUT

Output packet returned by the GRADD to the caller of the GHI_CMD_VRAM function.

    typedef struct _VRAMALLOCOUT {

      ULONG      ulLength;         /*  Size of the VRAMALLOCOUT data structure, in bytes. */

      ULONG      ulFlags;          /*  Flag indicating type of VRAM allocation. */

      ULONG      ulID;             /*  ID returned on allocation. */

      POINTL     ptlStart;         /*  X and Y location of VRAM. */

      ULONG      ulSize;           /*  Requested size of VRAM, in bytes. */

      ULONG      ulScanLineBytes;  /*  Length of scan line, in bytes. */

    } VRAMALLOCOUT;

    typedef   VRAMALLOCOUT   * PVRAMALLOCOUT ;