## Pen for OS/2 Device Driver Reference

[prev][next][parent][TOC]

### Set Locator Offset - Function 50h

Category 91, Locator IOCtls - Set Locator Offset

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Remarks

    #define PEN_FUNC_SLO 0x050

This function is used to change the finger offset of the digitizer. An offset can be negative. Both or either offsets can be changed according to the functions ORed in the command field.