## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### DEVESC_SWITCHBANK 33030l

This escape is handled by SwitchBank(ULONG cInCount, PULONG pInData). The pInData function is a pointer to a bank number. SwitchBank validates that the requested bank number is reasonable, saves it in the cursor_data structure to be restored by the cursor interrupt handler, and then sets the bank.