## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Examples

    Number   STRUC
       One    DB   1
       Two    DW   2
    Number   ENDS

       ;   The   following   line   is   only   allowed   in   MASM   5 . 10   mode   ( OPTION   OLDSTRUCTS )

       MOV   AX , [ BX ] . Two         ;   BX   points   to   a   " Number " ,   get   the   " Two "   entry

       ;   In   other   modes ,   " Two "   is   private   to   the   " Number "   structure   type ,   so
       ;   one   of   the   following   methods   are   required :

       MOV   AX , ( Number   PTR   [ BX ] ) . Two           ;   Explicit   override
       MOV   AX , [ BX ]   +   Number . Two                ;   Fully   qualified   reference
       ASSUME   BX : Number                         ;   Associate   BX   with   " Number "
       MOV   AX , [ BX ] . Two                          ;     then   original   syntax   is   allowed