## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### BIDI_Q_CONVERTER_INFO(8021h)

BIDI_Q_CONVERTER_INFO(8021h) gets protocol converter information.

This function returns information about the protocol converter currently active for the printer. If an extension protocol converter is being used, the extension should call the base converter to get the information about the base converter. The extension converter should then copy the base converter version and strings into the caller's buffer, along with the extension's information.