## Physical Device Driver Reference

[prev][next][parent][TOC]

### ASYNC_SETBREAKOFF (45h) - Remarks

If a general failure is not returned, then the physical device driver stops generating a break signal. It is not considered an error if the physical device driver is not generating a break signal. The physical device driver then resumes transmitting characters, taking into account all the other reasons why characters might be transmitted.