## Pen for OS/2 Device Driver Reference

[prev][next][parent][TOC]

### Resource Utilization

The sample pen device driver uses statically allocated memory in its device driver data segment. You can allocate dynamic memory, but this is not required by the device driver model. There will be no per-process data requirements.

Resources required by the device objects are similar to all Workplace Shell objects.