## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplProtXlateCmd Return Value - rc

rc (ULONG) - returns Return codes.

0 Success

8(ERROR_NOT_ENOUGH_MEMORY) Not enough memory to satisfy request.

87(ERROR_INVALID_PARAMETER) An invalid parameter was specified; most likely an invalid buffer pointer was given.

211(ERROR_INFO_NOT_AVAIL) The caller set PD_NEXTALERT. However, the protocol converter does not have any more alerts to return for the previous data passed to SplProtXlateCmd for the port.

234(ERROR_MORE_DATA) Part of the information requested was returned, but there was not enough room for all the data. *pcbOutData contains the size of buffer needed to retrieve all the query response data.

2123(NERR_BufTooSmall) No information was returned because the output buffer was too small. *pcbOutData contains the size of buffer needed to retrieve all the query response data.