## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreQueryColorIndex Parameter - flOptions

flOptions (ULONG) - input Options flag.

The only valid option is:

LCOLOPT_REALIZED If set, the information is required when the logical color table (if any) is realized. Otherwise, the information is required when the logical color table is not realized.

Other flags are reserved and must be 0.