## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### InnerGre Entries

The InnerGre entries are important to some 32-bit hardcopy presentation drivers that are coded in the "shadow DC" style. A shadow DC is actually a display OD_MEMORY DC. It is created by a printer driver to "steal" rasterization services from the currently installed display driver, and therefore save writing some code.