## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplStdGetBits

Select an item:

    Syntax
    Parameters
    Returns
    Remarks
    Glossary

Description:

SplStdGetBits transfers data from the identified PM_Q_STD buffer into a buffer owned by the presentation driver.

    #include <os2.h>

    HSTD    hstd;      /*  The handle to PM_Q_STD data. */

    LONG    lStart;

    LONG    cBytes;    /*  The number of bytes to transfer. */

    PCH     pAddress;

    BOOL    fSuccess;  /*  Return codes. */

    fSuccess = SplStdGetBits(hstd, lStart, cBytes,

                 pAddress);