## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Hardware Scissoring

Most of the routines in the driver do not use the S3 driver's scissoring capability. All of the routines assume, however, that initially the scissors are set so all memory is accessible. Therefore, hardware scissoring is implemented and any routines that use it should re-open the scissors after using them.