## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### VDHDecodeProperty Return Value - rc

rc (BOOL) - returns

Success If the function is successful, it returns a nonzero value and the ppProperty pointer is modified to point to the next range in the property string. StartNumberPtr and EndNumberPtr will have the range values. ppProperty is returned NULL after processing the last range.

Failure If the function fails, it returns 0, indicating an invalid parameter. If BaseFlag contains an invalid value or if ppProperty is NULL, a system halt occurs.