## Printer Device Driver

[prev][next][parent][TOC]

### SaveINIGroupData

This function appends a given string to a buffer in the following format:

    STRING11,STRING12,...STRING1N;STRING21,STRING22,...,STRING2N;...

If a string is provided, a comma is first appended to the end of the buffer to separate the new string. The string is then appended to the buffer. If no string is provided, the semicolon is appended to the string, thereby separating the groups of strings from other groups. The above string is NULL-terminated.