## Using Your DDK

[prev][next][parent][TOC]

### OEM SVGA Utility

Driver Description:

The OEM SVGA Utility consists of an executable file called SVGA.EXE. This executable generates a generic PMI file with a call to OEMPMI.DLL to set the mode using BIOS INT 10 calls.

Compilers/Assemblers Required:

         Microsoft MASM 5.1  (supplied with the DDK)
         Microsoft C 6.0

Build Instructions:

1.Ensure the necessary compilers and assemblers are installed.

2.Run the SETCMPLR.CMD REXX command file located in the DDK\TOOLS directory. This command initializes environment variables to be used during the build.

e.g., SETCMPLR <MSCpath> <VACpath> <CSETpath> <DDKpath>

    Where <MSCpath> represents the Microsoft C 6.0 install directory
           <VACpath> represents the IBM Visual Age C++ install directory
           <CSETpath> represents the IBM C Set ++ install directory
           <DDKpath> represents the DDK install directory

Note: A period (.) may be substituted for a compiler directory that is not used during the build.

3.Change the directory to DDK\VIDEO\SRC\VIDEO\OEMPMI\SVGAUTIL.

4.Invoke NMAKE on the resident makefile.

Files Created by Successful Build:

         Directory:  \DDK\VIDEO\REL\OS2C\RETAIL\BASE\OS2

         o  SVGAOEM.EXE