## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Generic Video Configuration Interface

The Video Configuration Manager supports a generic video configuration interface that allows any display driver to interface with the user via notebook settings in the System icon. The driver needs to export DevEscape calls that identify the capability. The driver also needs to provide DevEscape calls that allow the VIDEOCFG to query the current value and notify the driver when the user sets the value. The DevEscape functions are invoked as Ring3. The method of recording the current setting, as well as default values, is at the driver's discretion.