## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Access Authorization

The physical ASYNC device driver does not prevent multiple processes from concurrently opening the same device name. The physical device driver uses standard file system contention control. An application or subsystem that needs exclusive access to the COM device will open it with access rights set to DENY_ANY. Inheritance of open handles, and sharing of the device among multiple opens, works in a manner similar to regular files.